



![A blue rectangle with white dots

Description automatically generated](data:image/png;base64,iVBORw0KGgoAAAANSUhEUgAAAm8AAACvAQMAAACRj6tWAAAAAXNSR0IArs4c6QAAAARnQU1BAACxjwv8YQUAAAADUExURQCpsBPeifYAAAAJcEhZcwAAIdUAACHVAQSctJ0AAAAlSURBVGje7cExAQAAAMKg9U9tDQ8gAAAAAAAAAAAAAAAAAB7VADYBAAG/IHNyAAAAAElFTkSuQmCC)

MULTIWASHTM PRO

CALL FOR A FREE DEMONSTRATION

0114 244 4592

rshgroup.co.uk

MULTIWASHTM PRO

A range of scrubber dryers that are simple to use, cost-effective and provide exceptional cleaning results after just one pass.

# SIMPLE



Easy to use,

manoeuvre and

maintain

# PRODUCTIVE\*

Giving a quicker and more effective clean than traditional cleaning methods, saving you time and

money

# BATTERY POWERED



4 LITRE TANK

Accessible and removable tank for fast filling, emptying and cleaning

EASY

Handle assembly is quick and easy to assemble to the base, ready for the machine to be used

ACCESSORIES

7 litre solution tank for greater productivity

Trolley allows for easy transportation

Side brush allows you to clean right

up to the edge

POWERFUL

Counter- rotating cylindrical brushes scrub and lift dirt, giving a more hygienic and deeper clean

VERSATILE

Effective on all floors

with brushes available for carpets, hard floors, escalators and

Run-time of up to

60 minutes giving excellent productivity and with no trailing cables, it

minimises the risk

of trips and slips

# FAST CHARGE

BATTERY

With a 2hr charge time and a quick change battery system, there will be minimum down time when


charging

# EFFICIENT

Wash, scrub and dry in just one pass, leaving floors ready to walk on in

seconds

SEE THE



entrance matting

# HYGIENIC

Tested in a certified

lab to remove

>99.99% of S. aureus,

E. coli, P. aeruginosa

and B. subtilis

bacteria

# \*PRODUCTIVITY

INFECTION CONTROL

With the addition of the steam, dirt and grime will be removed easier than traditional cleaning

methods

MULTIWASHTM PRO IN ACTION

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Model |  | Mop | MWPRO240 | MWPRO340 | MWPRO440 | MWPRO340-STEAM | MWPRO340-BATTERY |
| Theoretical | m2/h |  | 650 | 930 | 1150 | 930 | 930 |
| Practical | m2/h | 150 | 250 | 350 | 430 | 350 | 350 |

2 0114 244 4592 | [sales@rshgroup.co.uk](mailto:sales@truvox.com) 3



REV.03 - (0924)

Subject to conditions



EDUCATION

HEALTHCARE

HIRE

LEISURE

RETAIL

VETERINARY

Rubber Safety Hygiene (Group) Ltd

2 Enterprise Works

Hunsley Street

Sheffield

S4 8DY

sales@rshgroup.co.uk | 0114 244 4592 | www.rshgroup.co.uk

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Model  Product Code |  | MultiwashTM PRO 240  MWPRO240 | MultiwashTM PRO 340  MWPRO340 | MultiwashTM PRO 440  MWPRO440 | MultiwashTM PRO 340/ STEAM  MWPRO340-STEAM | MultiwashTM PRO 340/ BATTERY  MWPRO340-BATTERY |
| SPECIFICATIONS |  |  |  |  |  |  |
| Voltage AC (~) / Frequency | V/Hz | 230 / 50 | 230 / 50 | 230 / 50 | 230 / 50 | - |
| Charging Voltage AC (~) / Frequency | V/Hz | - | - | - | - | 100 - 240 / 50 - 60 |
| Battery voltage DC | V/Hz | - | - | - | - | 25.6 |
| Battery details | Ah | - | - | - | - | 12 |
| Motor power | W | 750 | 950 | 1150 | 950 | 328 |
| Brush width | cm | 24 | 34 | 44 | 34 | 34 |
| Brush speed | rpm | 650 | 650 | 650 | 650 | 400 |
| Brush pressure | g/cm2 | 220 | 190 | 170 | 190 | 170 |
| Productivity rate | m2/h | 250 | 350 | 450 | 350 | 350 |
| Sound pressure level | dB(A) | 69 | 69 | 71 | 69 | 69 |
| Solution tank capacity | l | 4 | 4 | 4 | 4 | 4 |
| Recovery tank capacity | l | 2 | 3 | 4 | 3 | 3 |
| Steam generator power | W | - | - | - | 1250 | - |
| Steam jet width | mm | - | - | - | 340 | - |
| Temerature of steam | °C | - | - | - | 100 | - |
| Run time | mins | - | - | - | - | 60 |
| Charge time | hrs | - | - | - | - | 2 |
| Dimensions (L x W x H) | cm | 39 x 35 x 111 | 39 x 45 x 111 | 39 x 55 x 111 | 39 x 45 x 111 | 39 x 45 x 111 |
| Weight | kg | 21.5 | 26.5 | 31 | 31 | 23.5 |
| Cable length | m | 12 | 12 | 12 | 12 | - |
| STANDARD ACCESSORIES | | | | | | |
| Standard brush - black (pack of 2) | | 90-0727-0000 | 90-0728-0000 | 90-0729-0000 | 90-0728-0000 | 90-0728-0000 |
| Battery |  | - | - | - | - | WL0272-1 |
| Charger (UK & Euro) |  | - | - | - | - | 04-4089-0000 |
| OPTIONAL ACCESSORIES | | | | | | |
| Soft brush - grey (pack of 2) |  | 90-0730-0000 | 90-0731-0000 | 90-0732-0000 | 90-0731-0000 | 90-0731-0000 |
| Hard brush - blue (pack of 2) |  | 90-0733-0000 | 90-0734-0000 | 90-0735-0000 | 90-0734-0000 | 90-0734-0000 |
| Escalator brush - blue (pack of 2) | | 90-1019-0000 | 90-1020-0000 | 90-1021-0000 | 90-1020-0000 | 90-1020-0000 |
| Standard side brush - black (1 required) | | 90-0722-0000 | 90-0723-0000 | 90-0724-0000 | 90-0723-0000 | 90-0723-0000 |
| Soft side brush - grey (1 required) | | 90-0842-0000 | 90-0845-0000 | 90-0848-0000 | 90-0845-0000 | 90-0845-0000 |
| Hard side brush - blue (1 required) | | 90-0843-0000 | 90-0846-0000 | 90-0849-0000 | 90-0846-0000 | 90-0846-0000 |
| Trolley |  | 05-4781-0000 | 05-4781-0000 | 05-4781-0000 | 05-4781-0000 | 05-4781-0000 |
| 7 litre tank |  | 90-0826-0000 | 90-0826-0000 | 90-0826-0000 | 90-0826-0000 | 90-0826-0000 |

A blue oval with white text

Description automatically generated